HKP-62 Hydroseeder

Applications

The machine can mix different materials like seeds, mulch, fertilizer, soil conditioner, adhesives, moisturizer, straw, fiber covering materials, yellow soil, red soil, sandy soil, clay, even big proportion, high and super concentration slurry materials.

So it is versatile, can be widely applied in spray planting permanent vegetation, spraying slurry, slope protection greening and erosion prevention, also in irrigation, fertilize, pesticide spraying and other daily care, soil improvement work.

If you’re controlling erosion, restoring distressed lands, planting professional-grade turf for golf courses, or just planting hundreds of new home lawns each year, We have the equipment that’s right for you!

Features:

Large working volume. The max 1600 gallons (6000L) can be chosen. What’s more, you can modify the size to fit your needs.

Exclusive engine. It is the main part that Hengrui HKP series hydroseeder different from others. The outlet pressure can achieve 1.6MPa . It has strong power and high efficiency even can delivery slurry.

Fast mixing jet agitation system. The machine mixer uses double mixing mode of vane mechanical agitation and cycling efflux agitation, to ensure that in the whole hydroseeding process, the slurry is in completely suspension and homogeneous state.

Patented technology. Our products have applied for nine patents for inventions, utility models of a patent.

Factory direct sales----Cheapest Price. Our company is a manufacturer direct marketing our products has already export to Singapore, South Africa, The Philippines, Germany and so on.

High solid content. The max solid content of HKP series can achieve 70%. Be able to transfer high-solids content of the media, such as slurry.

Parameter:

Model	HKP-62
Weight(kg)	4000
Dynamic System	Engine	Water-cooled Diesel Engine
Power(kw)	62
Tank Size	Max	1600gal(6000L)
Working	1400gal(5200L)
Material Type	All types of Hydroseeding Mulch----No Restrictions
Slurry Pump	Flow(m³/h)	40
Outlet Pressure(Mpa)	1.6
Agitation	Mechanical Agitation
Max Solid Content(%)	65
Max Granular Solids(mm)	20
Spraying Area /Tank(m2)	240
Spraying Time /Tank(min)	10(direct),18(with pipe)
Nozzles	Two circles caliber 30mm, 35mm, one fan caliber 30mm
Dimension (L*W*H)(mm)	5100*2000*2400
Max Range(m)	20
Extended range(with pipe)(m)	60